IBERT

In the IBERT Console, apply the following changes to the settings:

|  |  |
| --- | --- |
| Setting | Value |
| Loopback Mode | Near-End PMA |
| TX Data Pattern | PRBS 31-bit |
| RX Data Pattern | PRBS 31-bit |

Press the “BERT Reset” button to reset the IBERT counter. The latter are biased when the above settings are not set properly. Link GTX\_X0Y17 is unreliable.